Gas Counter Heavy Duty Griddles

Heavy duty gas counter griddles built on welded angle iron frame construction for strength and durability. Removable grease container is provided for easy cleaning. Standard model sizes are 12” (305 mm), 24” (610 mm), 36”(915 mm), 48”(1,219mm), 60” (1,524 mm) and 72”(1,829 mm). All counter models are range match when placed on our equipment stand.

Features

* 5/8” thick, highly polished steel plate.
* 11/2” (546 mm) working depth.
* 4” (101.5 mm) plate rail.
* Spatula width – 3 1/8” (79 mm) – grease trough.
* One heavy duty steel tube burner per 12” section.
* Burner rated at 30,000 BTUs per hour.
* Each 12” section is controlled by a manual valve
* Each 24” section is controlled by a thermostat
* Large capacity grease container with integral lid.